MK MODEL BX-3 DRY PAVER/BLOCK SAW WITH STAND

110V CORDED

• Portable and lightweight - 50 lbs.

• Exclusive motor filter protects motor from dust particle damage

• 8" x 8" x 16" cutting capacity

• Lockable trigger-operating switch in the handle to allow for ease of operation

• Carrying handle incorporated into arm

• Spring-loaded head, lockable in the down position

• Heavy-duty cast aluminum rolling conveyor cart

• Open-back design for large materials to pass through

• Includes 14" Diamond Blade and rip guide